**Mechanical shower panel**

Mechanical, aluminium

Top inlet, handset, aluminium

Reference: **791350**

Specification description

Shower panel with single control mixer and removable handset:

Anodised aluminium shower panel for wall-mounted, exposed installation.

Non-time flow mechanical shower mixer.

Sliding handset on chrome-plated rail with flexible.

Top inlet via in-line stopcocks.

M½" connections.

Concealed fixings.

Filters.

Shower panel suitable for people with reduced mobility.

30-year warranty.