**Pre-rinse set with mixer**

Without bib tap

Black flexible and scale-resistant hand spray

Reference: **5626**

Specification description

Complete pre-rinse set without bib tap.

Single hole deck-mounted mixer with slimline control lever.

Suitable for intensive use in professional kitchens.

Supplied with F3/8" flexible hoses and non-return valves.

Black hand spray with adjustable jet and 9 lpm flow rate at the outlet (ref. 433010).

Scale-resistant hand spray with shock-resistant tip.

Reinforced, food-grade black flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.