**Food-grade flexible hose for catering**

Black, L.1.20m

Reference: **433120CH**

Specification description

Black, reinforced food-grade flexible hose L. 1.20m:

PVC sheath on stress area.

Anti-torsion rotating nut.

Flexible hose will withstand temperatures up to 70°C and 5 bar maximum pressure.

Spare part for repairing pre-rinse set components.