**Recessed shower tray**

800 x 800mm

Reference: **150300**

Specification description

Recessed shower tray, 800 x 800mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

One-piece pressed shower tray, seam-free for easy maintenance and better hygiene.

Rounded internal corners for improved safety in the shower.

Drainage slope.

Supplied with 1½" waste and trap.

Non-slip surface.

CE marked. Complies with European standard EN 14527.

Weight: 7kg.

[Formerly ref: 0513030000]