**PMR recessed shower tray**

800 x 800mm

Reference: **150500**

Specification description

Recessed shower tray, 800 x 800mm.

Suitable for people with reduced mobility: slimline shower tray.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.5mm

Drainage slope.

Supplied with 1½" waste.

Non-slip surface.

CE marked. Complies with European standard EN 14527.

Weight: 8.5kg.

[Formerly ref: 0513050000]