**PMR recessed shower tray**

900 x 900mm

Reference: **150600**

Specification description

Recessed shower tray, 900 x 900mm.

Suitable for people with reduced mobility: slimline shower tray.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.5mm

Drainage slope.

Supplied with 1½" waste and trap.

Non-slip surface.

CE marked. Complies with European standard EN 14527.

Weight: 9.5kg.

[Formerly ref: 0513060000]