**Neck tube for TEMPOMATIC 4 and TEMPOFLUX recessed flush valves**

For standard urinal Ø 35mm

Reference: **752430**

Specification description

Neck tube for TEMPOMATIC 4 recessed urinal valves, recessed TEMPOFLUX urinals and standard urinals with Ø 35mm connection washer for supply.

30-year warranty.