**Surgical scrub-up trough with low upstand**

Polished satin 304 stainless steel - 1 service - "Hygiene+" Design

Without tap hole

Reference: **185020**

Specification description

Wall-mounted surgical scrub-up trough with 75mm upstand.

Suitable for hospitals and healthcare facilities.

Bacteriostatic 304 stainless steel. Polished satin finish. Stainless steel thickness: 1.2mm.

Length 700mm, 1 service. Without tap hole.

Smooth surface for easy cleaning.

"Hygiene+": reduces niches where bacteria can develop, concealed trap, easy to clean.

Drainage on the right. Without overflow. Supplied with fixing elements and 1"1/4 waste.

CE marked. Complies with norm EN 14296.

Weight: 15.6kg.

30-year warranty.