**HYGIÉNA waste**

Waste with concave grid

M1"1/4, short version

Reference: **6110**

Specification description

Hygienic washbasin waste, M1¼" with concave grid (no water retention).

Free flow, with no central screw (avoids scale deposits and reduces bacterial development).

Polished chrome-plated brass grid, chrome-plated ABS body.

Can be tightened: mini. 1mm, maxi. 2mm.

Complies with EN 274-1.

Washbasin waste with 30-year warranty.