**Wall-mounted pre-mounted set with mixer and telescopic spout**

With bib tap and telescopic spout

White hand spray with scale-resistant diffuser

Reference: **G6732**

Specification description

Complete pre-rinse set with bib tap suitable for intensive use in professional kitchens.

Wall-mounted mixer F3/4" with 150mm centres with:

- valve heads with control knobs.

- non-return valves integrated in the mixer.

Bib tap with telescopic, swivelling spout L. 200 - 290mm.

- 20 lpm flow rate at the outlet.

- valve head with control knob.

White hand spray with adjustable jet and 10 lpm flow rate at the outlet (ref. 433003).

Scale-resistant hand spray with shock-resistant tip.

Reinforced, food-grade, white flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.