**Wall-mounted pre-rinse set with mixer**

Without bib tap

White flexible and scale-resistant hand spray

Reference: **G6733**

Specification description

Complete pre-rinse set without bib tap suitable for intensive use in professional kitchens.

Wall-mounted mixer F3/4" with 150mm centres with:

- valve heads with control knobs.

- non-return valves integrated in the mixer.

White hand spray with adjustable jet and 10 lpm flow rate at the outlet (ref. 433003).

Scale-resistant hand spray with shock-resistant tip.

White, reinforced, food-grade flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.