**HYGIÉNA basin waste**

Matte black waste with concave grid

M11/4", short model

Reference: **6110BK**

Specification description

Hygienic washbasin waste, M1¼" with concave grid (no water retention).

Free flow, with no central screw (avoids scale deposits and reduces bacterial development).

Brass grid with polished chrome-plated Teflon® finish and chrome-plated ABS body.

Can be tightened: min. 1mm, max. 2mm.

Conforms to EN 274-1.