**UNITO wall-mounted washbasin**

Matte black 304 stainless steel

Reference: **121830BK**

Specification description

Wall-mounted washbasin, 395 x 400mm.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm.

Matte black Teflon® finish.

Rounded edges prevent injury.

With Ø 35mm central tap hole.

Supplied without waste. Waste with black finish can be added (6110BK) or chrome finish (6110).

Without overflow.

CE marked. Complies with European standard EN 14688.

Weight: 3.6kg.

30-year warranty.