**Ø35mm ceramic cartridge**

Cartridge with base

Reference: **NSB262**

Specification description

Ø35mm standard ceramic cartridge with base and centering ring.

Cartridge with flow rate limited to 5 lpm.

For product ranges 2620/2621.