**Ø40mm ceramic cartridge**

Cartridge with base

With flow rate limiter

Reference: **N009AG75**

Specification description

Ø40mm standard ceramic cartridge with base, with flow rate limiter.

For deck-mounted basin mixer ranges:

- 2820L, 2820T (models sold before 05/2023)

- 2821L, 2821T

- 2720L, 2720T / 2721L, 2721T (models sold before 12/2022)

- 2520, 2520L, 2520T / 2521, 2521L, 2521T

For wall-mounted basin mixer ranges:

- 2445, 2446, 2455, 2456