**Solenoid valve**

For TEMPOMATIC 4 urinals and recessed BINOPTIC taps

MM1/2" - 6V

Reference: **430646**

Specification description

Solenoid valve.

For TEMPOMATIC 4 urinals and recessed BINOPTIC taps.

Union MM1/2".

Works with a 6V power supply.

Dimensions: 67mm.