**Control Plate**

For TEMPOMATIC WC dual control

Mains supply - Satin polished stainless steel

Reference: **464PISS**

Specification description

Control cover plate only with integrated electronic module.

For cistern-less flush TEMPOMATIC dual flush system.

230/6V mains supply.

Polished satin stainless steel cover plate with chrome-plated push-button.