**Time flow cartridge**

For TEMPOSOFT 2 basin mixers/taps

Time flow ~15 seconds

Reference: **743742**

Specification description

Time flow cartridge for TEMPOSOFT 2 basin mixers.

Time flow ~15 seconds.

Flow rate can be adjusted from 1.4 to 6 lpm.