**Flow straightener**

For TEMPOSTOP, TEMPOSOFT 2 and TEMPOMIX 3

In Hostaform®

Reference: **BJ13V**

Specification description

Flow straightener.

For TEMPOSTOP, TEMPOSOFT 2 and TEMPOMIX 3.

In Hostaform®.

Diameters: interior Ø13, exterior Ø14.5.