**Locking kit**

For sequential thermostatic basin mixer

Reference: **96SEF**

Specification description

Locking kit for sequential thermostatic basin mixer.

Locking kit for product range H9600 and H9605.

Locking kit with threaded rods L.75 mm.