**BINOPTIC deck-mounted electronic soap dispenser**

Liquid soap, foam soap or hydroalcoholic gel dispenser

Mains, satin finish 304 stainless steel, 1L tank

Reference: **512021S**

Specification description

Deck-mounted electronic soap dispenser.

Liquid soap, foam soap or hydroalcoholic gel dispenser.

No manual contact: infrared cell detects hands automatically.

Satin finish 304 stainless steel spout.

No waste pump dispenser.

Separate electronic unit and removable tank for installation beneath the washbasin.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with maximum viscosity of 3,000 mPa.s or specific foam soap.

Compatible with hydroalcoholic gel.

Total spout length: 105mm.

Supplied with 1 litre tank.

BINOPTIC electronic soap dispenser with 30-year warranty.

CE marked.