**Time flow cartridge**

TEMPOSTOP cartridge for urinals

~7 second time flow

Reference: **743528**

Specification description

TEMPOSTOP time flow cartridge for urinals.

For ¾" urinals.

With push-button.

~7 second time flow.

Flow rate can be adjusted.