**Time flow cartridge**

Mechanism for TEMPOCHASSE WC

Time flow ~7 sec.s

Reference: **743605**

Specification description

Time flow cartridge for TEMPOCHASSE WC valve.

For recessed or cross wall 1 1/4" WC valves.

Time flow ~7 seconds.