**Time flow cartridge**

Cartridge for TEMPOSTOP for basins and urinals

~3 second time flow

Reference: **743323**

Specification description

TEMPOSTOP time flow cartridge for basin taps and urinals.

Original version.

For basin taps with lever control.

For ¾" urinals.

~3 second time flow.

Flow rate can be adjusted.