**Time flow cartridge**

For TEMPOSTOP basin/urinal

Time flow ~7 seconds, AB anti-blocking system

Reference: **743105**

Specification description

Time flow cartridge for TEMPOSTOP basin/urinal.

Time flow ~7 seconds.