**TEMPOMATIC 4 electronic soap dispenser**

Liquid soap, foam soap or hydroalcoholic gel dispenser

Mains supply, chrome-plated, 1L tank

Reference: **512041P**

Specification description

Wall-mounted electronic soap dispenser.

Liquid soap, foam soap or hydroalcoholic gel dispenser.

No manual contact: hands are automatically detected by infrared cell.

Spout made from chrome-plated 304 stainless steel.

No waste dose dispenser.

Separate electronic unit and removable tank for installation under the basin.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s or specialist foam soap.

Compatible with hydroalcoholic gel.

Spout length: 112 mm.

Supplied with a 1 litre tank.

Electronic soap dispenser with 30-year warranty.

CE marked.