**Wall-mounted black AQUEDUTO washbasin**

Matte black 304 stainless steel - With concealed drainage

Without tap hole

Reference: **120150BK**

Specification description

Wall-mounted washbasin, 700 x 440mm.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm.

Matte black Teflon® finish.

Rounded edges prevent injury.

Without tap hole.

Supplied with 1¼" waste.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 12kg.

30-year warranty.