**Hygienic scale-resistant flow straightener**

For 262x range

M24/100

Reference: **927024**

Specification description

Scale-resistant flow straightener.

Flow rate set at 4 lpm at 3 bar.

Flow straightener with no grid: reduces bacterial development, no water retention or scale deposits.

M24/100.

Supplied as a single unit.

30-year warranty.