**Cartouche céramique Ø40**

Cartridge without base

With flow rate limiter 9 lpm

Reference: **N249AA75**

Specification description

Ø40mm standard ceramic cartridge without base, flow rate limiter 9 lpm.

Cartridge for ranges - 2210, 2510.